**Hardware Specification**

If portable ELD, ELD need to be fix mounted in a fixed position during operation of motor vehicle and visible to seated driver in the normal driving position.