**Misc Specification**

* User’s manual for how to operate the ELD
* Instruction sheet for the driver describing the data transfer mechanisms supported by the ELD and step-by-step instructions for the driver to produce and transfer the driver’s HOS records to authorized safety official.
* Instruction sheet for the driver describing ELD malfunction reporting requirements and recordkeeping procedure during ELD malfunctions
* Blank Driver Daily Logs for minimum of 8 days.
* Driver must note malfunction of ELD and report to motor carrier within 24 hours
* Driver must have previous 7 days of duty status on graph-grid paper logs or retrievable from ELD.
* Driver must continue to prepare a record of duty status manually until the ELD is serviced and brought back into service
* Driver must know how to resolve diagnostic event according to ELD provider’s recommendation.
* Motor carrier must take actions to correct malfunction with 8 days of knowing, if more time is required then motor carrier must apply to FMCSA and FMCSA will review on case by case basis.